\*\* NOTE TO SPECIFIER \*\* Standalone digital keypads for single doors with multiple user with individual PIN codes. Delete if not required.

* + 1. Digital Keypad, Integrated:
       1. Product: Model 918 Indoor EntryCheck as manufactured by SDC.

Single gang keypad with 500 users. User Codes to be 4 to 6 digits in length, programmable for individual or simultaneous control of 2 relay outputs momentary, timed or latching with 2 additional programmable solid state outputs

* + - * 1. Two LEDs - Output Red/Green and Amber status indicators.
        2. Four Outputs: Relay #1, SPDT, 5 Amps at 30 V. Relay #2, SPDT, 2 Amp at 30 V. Output #3 and #4, solid state open collectors 100 mA at 24 VDC.
        3. Voltage: 12/24 VDC or AC (AC supply shall be transformer isolated).

Current: 30 mA typical, 150 mA maximum.

* + - * 1. Automatic time-out REX input,
        2. Choice of function for Sense input - Keypad disable or Door Sense
        3. Forced Entry
        4. Door ajar
        5. Inhibit Relay 1 or 2
        6. Auto relock when door closes
        7. Choice of function for Relay #2 and two solid state outputs #3 & #4

1. Alarm shunt
2. Forced entry
3. Door ajar
4. Tamper lockout
5. Keypad active
   * + - 1. Timed Anti-tailgate
         2. Blue illuminated keys with tactile feel
         3. Single gang Stainless Steel plate or plated finishes (4.75”Hx 3.00W”x 1.5”D)
       1. Finish: U - 630 Stainless Steel (Std)
       2. Finish: C - 605 Bright Brass (Opt)
       3. Finish: D - 606 Dull Brass (Opt)
       4. Finish: H - 613 Oil Rubbed Bronze (Opt)
       5. Finish: P - 625 Bright Chrome (Opt)
       6. Optional - Provide Plug in Power Supply: Model TR12 as manufactured by SDC Security Door Controls.