Narrow Style Digital Keypad, Integrated, Indoor /Outdoor:

* + - 1. Product: Model 923 Narrow Style Indoor/Outdoor EntryCheck as manufactured by SDC. Narrow style keypad with 500 users. User Codes to be 4 to 6 digits in length, programmable for individual or simultaneous control of 2 relay outputs momentary, timed or latching with 2 additional programmable solid state outputs
         1. Two LEDs - Output Red/Green and Amber status indicators.
         2. Four Outputs: Relay #1, SPDT, 5 Amps at 30 V. Relay #2, SPDT, 2 Amp at 30 V. Output #3 and #4, solid state open collectors 100 mA at 24 VDC.
         3. Voltage: 12/24 VDC or AC (AC supply shall be transformer isolated). Current: 30 mA typical, 150 mA maximum.
         4. Automatic time-out REX input,
         5. Choice of function for Sense input - Keypad disable or Door Sense
         6. Forced Entry
         7. Door ajar
         8. Inhibit Relay 1 or 2
         9. Auto relock when door closes
         10. Choice of function for Relay #2 and two solid state outputs #3 & #4

1. Alarm shunt
2. Forced entry
3. Door ajar
4. Tamper lockout
5. Keypad active
   * + - 1. Timed Anti-tailgate
         2. Blue illuminated keys with tactile feel
         3. Narrow style rugged cast housing (7.3125”Hx 1.75”Wx 1.375”D)
         4. Operating Temperature; -4 degree F to +140 degree F (-20 degree C to +60 degree C).
         5. Humidity: 5% to 95%, non-condensing.