* + 1. Digital Keypad, Integrated, Outdoor:

Product: Model 926 /Outdoor EntryCheck as manufactured by SDC. Keypad mounted in rugged steel housing with key lock front cover. Pedestal, post or surface mountable. Numeric keypad with 500 user codes. User Codes to be 4 to 6 digits in length and programmable for individual or simultaneous control of 2 SPDT relay outputs - momentary, timed or latching with 2 additional programmable solid state outputs

* + - * 1. Two LEDs - Output Red/Green status indicator and Amber programming status indicator.
        2. Four Outputs: Relay #1, SPDT, 5 Amps at 30 V. Relay #2, SPDT, 2 Amp at 30 V. Output #3 and #4, solid state open collectors 100 mA at 24 VDC.
        3. Voltage: 12/24 VDC or AC (AC supply shall be transformer isolated).

Current: 30 mA typical, 150 mA maximum.

* + - * 1. Automatic time-out REX input,
        2. Choice of function for Sense input - Keypad disable or Door Sense

1. Forced Entry
2. Door ajar
3. Inhibit Relay 1 or 2
4. Auto relock when door closes
   * + - 1. Choice of function for Relay #2 and two solid state outputs #3 & #4
5. Alarm shunt
6. Forced entry
7. Door ajar
8. Tamper switch activated
9. Keypad active
   * + - 1. Timed Anti-tailgate
         2. Blue illuminated keys with tactile feel
         3. Rugged steel housing with key lock front cover (6-3/8”H x 4-3/4”W x 4-1/2”D)
         4. Pedestal, post or surface mountable
         5. Suitable for outside gate operators
         6. Operating Temperature; -4 degree F to +140 degree F (-20 degree C to +60 degree C).
         7. Humidity: 5% to 95%, non-condensing