* 1. MOTORIZED LATCH RETRACTION MORTISE LOCKSETS
     1. ANSI Grade 1 Heavy Duty – Motorized Latch Retraction Mortise Lockset:
        1. Product: MLR Z7600 - Motorized Latch Retraction Mortise Lockset as manufactured by SDC Security Door Controls.
           1. UL Listed for 3 hour fire rated doors.
           2. Failsecure.
           3. Field selectable function: Locked outside only or both sides.
           4. Motorized Low current operation
           5. 620 mA inrush, 160 mA holding current @ 24vdc
           6. Field selectable handing.
           7. Compatible with Automatic Door operator applications
           8. Replaces most major brands of mechanical mortise locks for new or retrofit applications.

\*\* NOTE TO SPECIFIER \*\* Delete function not required.

* + - 1. Function: Z7632 Failsecure, locked both sides.
      2. Function: Z7652 Failsecure, locked outside only.

\*\* NOTE TO SPECIFIER \*\* Handing: Delete handing not required.

* + - 1. Handing: L - Left hand.
      2. Handing: LR - Left hand reversed.
      3. Handing: R - Right hand.
      4. Handing: RR - Right hand reversed.

\*\* NOTE TO SPECIFIER \*\* Finish Q standard. Delete finish not required.

* + - 1. Finish: C - 605 Bright Brass.
      2. Finish: D - 606 Dull Brass.
      3. Finish: F - 611 Bright Bronze.
      4. Finish: G - 612 Dull Bronze.
      5. Finish: H - 613 Oil Rubbed Bronze.
      6. Finish: P - 625 Bright Chrome.
      7. Finish: Q - 626 Dull Chrome (Standard)
      8. Finish: S - 629 Bright Stainless Steel.
      9. Order complete with SDC Trim or Less Trim. Compatible with Schlage Trim provided by Others.

\*\* NOTE TO SPECIFIER \*\* Lever Trim: Delete trim not required.

* + - 1. SDC Lever Trim: G - Galaxy with rose.
      2. SDC Lever Trim: GE - Galaxy with escutcheon.
      3. SDC Lever Trim: E - Eclipse with rose.
      4. SDC Lever Trim: EE - Eclipse with escutcheon.
      5. SDC Lever Trim: N - Nova with rose.
      6. SDC Lever Trim: NE - Nova with escutcheon.
      7. SDC Lever Trim: 07 - Schlage equivalent 07 with SDC B rose.
      8. SDC Lever Trim: 07E - Schlage equivalent 07 with SDC escutcheon.

\*\* NOTE TO SPECIFIER \*\* Delete options not required.

* + - 1. Options/Suffix: R - Request-to-exit Output, SPDT. 5A @ 30vdc
      2. Options/Suffix: LM – Latchbolt Status Output, SPDT.5A @ 30vdc
      3. Mortise Key Cylinder Option – 1 Required for Z7652; 2 Required for Z7632

\*\* NOTE TO SPECIFIER \*\* Keyed Cylinder: Delete cylinder not required.

* + - 1. Keyed Cylinder Optional: CYL-6KDQ - 6 pin, 1.125 inches (29 mm) mortise cylinder, keyed different, dull chrome.
      2. Keyed Cylinder Optional: CYL-6KAQ - 6 pin, 1.125 inches (29 mm) mortise cylinder, keyed alike, dull chrome.